|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **IMS drawing no.** | **Date of issue** | **Rev.** | **IMS purchasing dep. – KLE** | **Phone** | **Fax** |
| **Supplier** | **IMS quality – TQT** | **Phone** | **Fax**Sample |
| **Supplier sales department** | **Phone** | **Fax** |
| **Supplier quality department** | **Phone** | **Fax** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **No.** | **Measure** | **[x]  required** | **Comments** | **Checked** |
| 1 | Feasibility study | **with offer** | Use attached [Form-CS-172b](https://cms.imscs.com/sites/default/files/download-center/Form-CS-172b-Feasibility_Statement.doc) |   |
| 2 | Estimated capacity | **with offer** |   |   |
| 3 | Process FMEA | [ ]  |   |   |
| 4 | Control plan | [x]  |   |   |
| 5 | Test equipment capability (gauge R&R) | [ ]  |   |   |
| 6 | Capability of machine / tool (short-term capability):cm, cmk values: dimensions with ; 50parts | [ ]  |   |   |
| 7 | Initial sample test report:All dimensions and specifications including material certificates + reference samples filed by supplier | [x]  |   |   |
| 8 | Material certificate according to ISO 10474 or DIN EN 10204:3.1B | [ ]  |   |   |
| 9 | Material declaration - IMDS | [x]  |   |   |
| 10 | Coating-thickness measuring report | [x]  |   |   |
| 11 | Reference sample | [x]  |   |   |
| 12 | Preliminary process capability: pp, ppk values: dimensions with ◇min. 10 random samples (n=5) / min. interval 0.5h (other intervals after consultation with IMS)  | [ ]  |   |   |
| 13 | Proof of process capability: * cp, cpk values: Dimensions with ◇

 50 random samples (n=5) / min 50h* Capacity and frequency of defects
 | [ ]  |   |   |
| 14 | SPC monitoring: Dimensions marked with SPCReference sample comp. with series | [ ]  |   |   |

|  |
| --- |
| All measures must be completed according to the IMS specifications and requirements. |
| Signature quality manager of supplier | Date |

|  |
| --- |
| Series approval for product |
| Signature IMS-TQT | Date |

Comments:

**Double border = to be completed by supplier**

Documents regarding items 1 and 2 must be forwarded by the supplier together with the offer to the purchasing department of IMS Connector Systems. Steps 3 to 14 become only relevant in the event of an order by IMS-CS. Send the completed form together with the order confirmation to the purchasing department of IMS-CS.